[bookmark: _GoBack]1.Enter in the Setting menu, input the password:1512,then the XCAM Setup menu will be displayed,


2.Enter in the XCAM Setup menu:

  
3. And enter in the DQCAM menu, the DQCAM ON/OFF set to On.

 
4. Press Active button.
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